TECHNICAL SPECIFICATION  TYRRELL YAMAHA 024
-----------------------------------------------------------

CHASSIS
-----------------------------------------------------------
Construction        - Moulded carbon fibre and honeycomb
                      composite structure to fully meet the
                      FIA 1996 strength and impact
                      regulations 

Front Suspension    - Combined spring and damper units
                      operated by push rods and rockers,
                      third spring,mechanical anti-roll bar 

Rear Suspension     - Combined spring and damper units
                      operated by push rods and rockers,
                      third spring,mechanical anti-roll bar 

Dampers             - Koni 
Wheels              - Fondmetal cast magnesium:
                      Front 4-spoke, 11.5 in wide,
                      Rear 5-spoke, 13.7 in wide 

Fuel and Lubricants - Elf 
Tyres               - Goodyear 
Brakes              - AP Racing:
                      Front 2 x 6 piston calipers,
                      Rear 2 x 4 piston calipers 

Brake Discs & Pads  - Hitco carbon supplied by AP Racing 
Pipe Systems        - Titeflex 
Steering            - Tyrrell rack and pinion 
Steering Wheel      - Personal 
Driver's Seat       - Anatomically formed carbon composite 

Seat Belts          - Willans 6-point harness
                      (75 mm wide shoulder straps) 

Extinguisher        - Tyrrell carbon fibre moulded tank to
                      FIA 1996 specification, pressure
                      filled with Spraylance AFFF
                      extinguishant. 

Fuel Tank           - ATL Kevlar bladder to FIA FT5
                      specification 
Battery             - Tyrrell 12v 5Ah lead acid 
Instrumentation     - Pi Research System V, integrated
                      digital data display and telemetry. 

ENGINE 
-----------------------------------------------------------
Type                - Yamaha OX11A V-10 3-litre 
Injection/Ignition  - Zytek 
Spark Plugs         - NGK 

TRANSMISSION 
-----------------------------------------------------------
Gearbox             - Tyrrell longitudinal three-shaft
                      6-speed unit 
Gear selection      - Pneumatic, sequential 
Drive Shafts        - Tyrrell 
Clutch              - AP Racing carbon plate 
Differential        - Tyrrell / X-Trac viscous coupling 

DIMENSIONS 
-----------------------------------------------------------
Overall length      - 4430 mm Wheelbase 2940 mm 
Front track         - 1700 mm Rear track 1610 mm 
Overall width       - 2000 mm Height 950 mm 

-----------------------------------------------------------
Source: Tyrrell Racing Organization
-----------------------------------------------------------