-----------------------------------------------------------
Technical specifications - Ferrari 412T1             (1994)
-----------------------------------------------------------

Engine                   - Ferrari 3500 (F4 A 94)
Fuel and lubricants      - Agip Petroli
Number of cylinders      - 12 in 65° V
Number of valves         - 48

Capacity                 - 3,497.96 cc
Max. power output        - Over 700 bhp
Fuel feed                - Magneti Marelli digital
                           electronic injection.

Sparkplugs               - Champion dia. 10 mm
Electronic ignition      - Magneti Marelli solid state
Drive                    - Rear

Gearbox control          - Semiautomatic sequential with
                           electronic control
Number of speeds         - 6 + Reverse

Brakes                   - on all four wheels, ventilated
                           carbon discs

Gearbox and differential - Transverse Ferrari, self-locking
                           differential.

Suspension               - Independent with strut springing
                           front and rear.

Chassis                  - Composite, honeycomb with carbon
                           fibre.

Length                   - 4,495.5 mm
Width                    - 1,995 mm
Height                   - 995 mm
Front track              - 1,690 mm
Rear track               - 1,605 mm
Wheelbase                - 2,950 mm
Weight                   - 505 kg (with water and oil)
Rims                     - BBS 13" front and rear
Tyres                    - Goodyear
Official sponsors        - Marlboro, Fiat, Pioneer
Other suppliers          - Riv Skf, Arexons, Usag,
                           Trw Sabelt, Momo, Digital

-----------------------------------------------------------
Source: Ferrari
-----------------------------------------------------------