-----------------------------------------------------------
Technical characteristics of the Jordan Peugeot 196
-----------------------------------------------------------

CHASSIS
-----------------------------------------------------------
Single shell entirely made of composite carbon fibres.

FRONT SUSPENSION
-----------------------------------------------------------
Power connecting rods in composite fibres, working two
Jordan GP shock absorbers, drawn in unequal-length
triangles with the upper triangle in composite material and
the lower triangle in steel; the arms are built in steel,
as is the front roll-bar. 

REAR SUSPENSION
-----------------------------------------------------------
Power connecting rods in composite material working two
double Jordan GP shock absorbers mounted on the 
transmission-box with unequal-length triangles, with arms
and rear anti-roll bar in steel. 

TRANSMISSION COLUMN
-----------------------------------------------------------
In-house design Seven speed (plus reverse) longitudinal
gearbox Electronically-piloted sequential control for gear
changes. 

CLUTCH
-----------------------------------------------------------
Double-disc Tilton Racing system.

BRAKES
-----------------------------------------------------------
Brembo braking systems, front and rear metallic matrix
four-piston toe-links, discs and brake pads in SEP carbon. 

WHEEL RIMS
-----------------------------------------------------------
OZ Racing forged according to Jordan's specifications

TYRES
-----------------------------------------------------------
Goodyear

DIMENSIONS
-----------------------------------------------------------
Fuel tank capacity   145 liters
Wheelbase            2950 mm
Front width          1700 mm
Rear width           1618 mm
Overall height       950 mm
Overall length       4450 mm
Total weight         600 kg including the driver

-----------------------------------------------------------
Technical Specifications of the Peugeot V10 engine 
-----------------------------------------------------------

Number of cylinders:   10 in a V formation at 72°
Size:                  2998 cc.
Distribution:          Pinion cascades
Valves:                4 per cylinder with pneumatic recall
Cylinder block:        light-weight alloy
Drive shafts:          2 per cylinder row
Firing:                TAG Electronic Management
Dimensions (mm):       620 x 538 x 408
Weight:                133 kg.


-----------------------------------------------------------
Source: http://www.peugeot.com/
-----------------------------------------------------------