LIGIER-MUGEN HONDA JS41
-----------------------------------------------------------

ENGINE
-----------------------------------------------------------
Type                   Mugen Honda MF301
Cylinders              V10
Vee-angle              72°
Sparking plugs         NGK
Electronics            Honda PGM/FI
Fuel                   Elf
Oil                    Elf

TRANSMISSION
-----------------------------------------------------------
Gearbox                Benetton 6-speed transverse
Driveshafts            Ligier
Clutch                 AP

CHASSIS
-----------------------------------------------------------
Front suspension       Double wishbones, pushrod
Rear suspension        Double wishbones, pushrod
Suspension dampers     Dynamic/WP
Wheel diameter         Front 13 inch, rear 13 inch
Wheel rim widths       Front 11 inch, rear 16,5 inch
Tyres                  Goodyear
Brake pads             Carbone Industrie
Brake discs            Carbone Industrie
Brake calipers         AP/Brembo
Steering               Ligier
Radiators              Secan
Fuel tanks             ATL
Battery                FIAMM
Instruments            Ligier


DIMENSIONS
-----------------------------------------------------------
Weight                 1311,7 lb / 595 kg including driver
Wheelbase              115.7 inch / 2940 mm


-----------------------------------------------------------
Source: various car magazines