-----------------------------------------------------------
Technical Specifications - Ferrari 412T2             (1995) 
-----------------------------------------------------------

ENGINE
-----------------------------------------------------------
Type                   Ferrari 044
Cylinders              V12
Vee-angle              75°
Sparking plugs         Champion
Electronics            Magneti Marelli
Fuel                   Agip
Oil                    Agip

TRANSMISSION
-----------------------------------------------------------
Gearbox                Ferrari 6-speed transverse
Driveshafts            Ferrari
Clutch                 Daikin

CHASSIS
-----------------------------------------------------------
Front suspension       Double wishbones, pushrod,
                       torsion spring
Rear suspension        Double wishbones, pushrod,
                       torsion spring
Suspension dampers     Ferrari
Wheel diameter         Front 13 inch, rear 13 inch
Wheel rim widths       Front 12 inch, rear 13,7 inch
Tyres                  Goodyear
Brake pads             SEP and Hitco
Brake discs            SEP and Hitco
Brake calipers         Brembo
Steering               Ferrari
Radiators              Secan
Fuel tanks             ATL
Instruments            Magneti Marelli


DIMENSIONS
-----------------------------------------------------------
Weight                 1311,7 lb / 595 kg including driver
Wheelbase              115.3 inch / 2930 mm
Fuel capacity          27.4 gallons / 125 litres


-----------------------------------------------------------
Source: various car magazines