TYRRELL-YAMAHA 022
-----------------------------------------------------------

CHASSIS
-----------------------------------------------------------
Construction          Moulded carbon fibre and honeycomb
                      composite structure to meet the 1994
                      FIA specification

Front Suspension      Separate spring and dainper units
                      operated by push rods and rockers
Rear Suspension       Mechanical anti-roll bar
Suspension Dampers    Separate spring and damper units
                      operated by push rods and rockers

Wheels                Fondmetal
                      Front 3-spoke, 11.0 in wide
                      Rear 5-spoke, 13.7 in wide

Tyres                 Goodyear
Brakes                AP Racing
                      Front 2 x 6 piston calipers
                      Rear 2 x 4 piston calipers
Pipe systems          Titeflex
Steering              Tyrrell rack and pinion
Steering Wheel        Personal
Driver's seat         Anatomically formed carbon composite
Seat Belts            Willans / 6-point harness
Extinguisher          Tyrrell carbon fibre moulded bottle
                      to FIA 1994 specification.
Fuel Tank             Kevlar bladder to FIA FT5
                      specification
Battery               Tyrrell 12v 5Ah lead acid
Instrumentation       PI / Integrated digital data display
                      and telemetry

ENGINE
-----------------------------------------------------------
Type                  Yamaha OXlOA V-10
Injection/Ignition    Zytek
Fuel/Lubricants       BP
Spark Plugs           NGK

TRANSMISSION
-----------------------------------------------------------
Gearbox               Tyrrell transverse twin-shaft 6-speed
                      unit with pneuinatic sequential
                      selection
Drive Shafts          Tyrrell
Clutch                Triple carbon plate / AP Racing
Differential          Tyrrell

DIMENSIONS
-----------------------------------------------------------
Wheelbase             2900 mm
Front track           1700 mm
Rear track            1610 mm

-----------------------------------------------------------
Source: Tyrrell Racing Organization
-----------------------------------------------------------