McLAREN-MERCEDES MP4/10
-----------------------------------------------------------

ENGINE
-----------------------------------------------------------
Type                   Mercedes-Benz FO110
Cylinders              V10
Vee-angle              75°
Electronics            TAG Electronics
Fuel                   Mobil
Oil                    Mobil

TRANSMISSION
-----------------------------------------------------------
Gearbox                McLaren 6-speed transverse
Driveshafts            McLaren
Clutch                 Sachs

CHASSIS
-----------------------------------------------------------
Front suspension       Unequal length wishbones, pushrod,
                       inboard spring/damper
Rear suspension        Unequal length wishbones, pushrod,
                       inboard spring/damper
Suspension dampers     Bilstein
Wheel diameter         Front 13 inch, rear 13 inch
Wheel rim widths       Front 11,75 inch, rear 13,7 inch
Tyres                  Goodyear
Brake pads             Carbone Industrie or Hitco
Brake discs            Carbone Industrie or Hitco
Brake calipers         AP
Steering               McLaren
Radiators              McLaren/Calsonic
Fuel tanks             ATL
Battery                GS
Instruments            TAG Electronics

DIMENSIONS
-----------------------------------------------------------
Weight                 1311,7 lb / 595 kg including driver
Wheelbase              115.1 inch / 2925 mm
Track                  Front 66.5 inch / 1690 mm
                       Rear  63.1 inch / 1605 mm

-----------------------------------------------------------
Source: various car magazines