-----------------------------------------------------------
Technical Specifications  - Ferrari F310   (1996)
-----------------------------------------------------------

Model                     - F 310
Engine                    - 3000 Ferrari (046)
Fuel and lubricant        - Shell

Number of cylinders       - 10 in a 75° layout
Number of valves          - 40
Total displacement        - 2998.1 cc
Maximum power             - >600 HP

Fuel feed                 - Magneti Marelli digital
                            injection

Electronic ignition       - Magneti Marelli solid state
Drive                     - Rear

Gearbox control           - Semiautomatic sequential
                            electronically controlled

Number of speeds          -  6+reverse
Brakes on all four
wheels                    - Ventilated carbon disks

Gearbox and differential  - Ferrari transverse gearbox.
                            Limited slip differential

Suspension                - Independent, push-rod activated
                            torsion spring front and rear

Chassis                   - Carbon fiber and honeycomb
                            composite structure

Length                    - 4355 mm
Width                     - 1995 mm
Height                    - 970 mm

Front track               - 1690 mm
Rear track                - 1605 mm
Wheelbase                 - 2900 mm

Weight                    - 600 kg with water, lubricant
                            and driver

Wheels                    - 13" (front and rear)
Tyres                     - Goodyear

-----------------------------------------------------------
Source: Ferrari
-----------------------------------------------------------